Configuration	BTSP02
STM32CubeMX 	4.20.1
Date	02/07/2019
MCU	STM32F446RETx



PERIPHERALS	MODES	FUNCTIONS	PINS
ADC1	IN0	ADC1_IN0	PA0-WKUP
ADC1	IN1	ADC1_IN1	PA1
ADC1	IN10	ADC1_IN10	PC0
ADC1	IN11	ADC1_IN11	PC1
RCC	Crystal/Ceramic Resonator	RCC_OSC_IN	PH0-OSC_IN
RCC	Crystal/Ceramic Resonator	RCC_OSC_OUT	PH1-OSC_OUT
SYS	SysTick	SYS_VS_Systick	VP_SYS_VS_Systick
TIM1	Internal Clock	TIM1_VS_ClockSourceINT	VP_TIM1_VS_ClockSourceINT
TIM1	PWM Generation CH1	TIM1_CH1	PA8
TIM1	PWM Generation CH2	TIM1_CH2	PA9
TIM1	PWM Generation CH3	TIM1_CH3	PA10
TIM1	PWM Generation CH4	TIM1_CH4	PA11
TIM2	Internal Clock	TIM2_VS_ClockSourceINT	VP_TIM2_VS_ClockSourceINT
TIM3	Encoder Mode	TIM3_CH1	PC6
TIM3	Encoder Mode	TIM3_CH2	PC7
USART2	Asynchronous	USART2_RX	PA3
USART2	Asynchronous	USART2_TX	PA2
USB_OTG_HS	Host_Only	USB_OTG_HS_DM	PB14
USB_OTG_HS	Host_Only	USB_OTG_HS_DP	PB15



Pin Nb	PINs	FUNCTIONs	LABELs
2	PC13	GPIO_EXTI13	B1 [Blue PushButton]
3	PC14-OSC32_IN*	RCC_OSC32_IN	
4	PC15-OSC32_OUT*	RCC_OSC32_OUT	
5	PH0-OSC_IN	RCC_OSC_IN	
6	PH1-OSC_OUT	RCC_OSC_OUT	
8	PC0	ADC1_IN10	AUX2L
9	PC1	ADC1_IN11	AUX2R
14	PA0-WKUP	ADC1_IN0	AUX1L
15	PA1	ADC1_IN1	AUX1R
16	PA2	USART2_TX	USART_TX
17	PA3	USART2_RX	USART_RX
21	PA5	GPIO_Output	LD2 [Green Led]
35	PB14	USB_OTG_HS_DM	
36	PB15	USB_OTG_HS_DP	
37	PC6	TIM3_CH1	Encorder+
38	PC7	TIM3_CH2	Encorder-
39	PC8	GPIO_Output	LCD_Backlight
40	PC9	GPIO_Output	LCD_CS
41	PA8	TIM1_CH1	SPK1L+
42	PA9	TIM1_CH2	SPK1L-
43	PA10	TIM1_CH3	SPK1R+
44	PA11	TIM1_CH4	SPK1R-
46	PA13*	SYS_JTMS-SWDIO	TMS
49	PA14*	SYS_JTCK-SWCLK	TCK
51	PC10	GPIO_Output	LCD_SCK
52	PC11	GPIO_Output	LCD_A0
53	PC12	GPIO_Output	LCD_SDA
55	PB3*	SYS_JTDO-SWO	SWO



SOFTWARE PROJECT

Project Settings : 
Project Name : BTSP02
Project Folder : /Users/togashitoyohiko/Documents/OpenSTM32/BTSP02
Toolchain / IDE : SW4STM32
Firmware Package Name and Version : STM32Cube FW_F4 V1.16.0


Code Generation Settings : 
STM32Cube Firmware Library Package : Copy only the necessary library files
Generate peripheral initialization as a pair of '.c/.h' files per peripheral : No
Backup previously generated files when re-generating : No
Delete previously generated files when not re-generated : Yes
Set all free pins as analog (to optimize the power consumption) : No


Toolchains Settings : 
Compiler Optimizations : Balanced Size/Speed






